**Construction of a local road from the local road for the village of Banjica to the village of Otistino - Municipality of Chashka**

Total road length: L = 212 m

* Design speed: 30 km/h
* Road profile width: 4.50 m

**Pavement Structure**

* BNHS 16 – asphalt layer: d = 7cm

The subject street is part of Т4D5.

The work is being carried out by the construction DPTU ЕSKAVATORI – MK Dooel Skopje. The value of the signed contract is 2,846,182 denars.

**Project Overview**

**Preparatory work:**

* Securing and marking the route

**Lower and upper structure:**

* Mechanical excavation of earth in a wide excavation 3-4 floors.
* Subsoil preparation
* Embankment preparation (improved bed 15cm)
* Installation of buffer layer (under the roadway) d=30cm
* Installation of BNHS 16 layer d=7cm
* Construction of shoulders 1x0.5cm
* Construction of gutter d=0.5cm

**Traffic signals:**

* Installation of traffic signs

**Additional quantities:**

* Concrete curbs 18/24 (on the left side) for gutter

|  |  |
| --- | --- |
|  |  |
|  |  |
|  |  |
|  |  |